{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["WIRE04"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"WIRE04","index":0,"n_rows":624,"n_cols":11,"rows_kept":624,"cut":false,"hidden":false,"merged":[]}
["PIANO WIRE"]
[]
[null,null,"MATERIAL:  POLISHED SPRING STEEL"]
[null,null,"Specification:   BS  5216   ND3"]
[]
["SIZE",null,null,null," SALES PRICE PER KILO"]
["MM","S.W.G.","PART NO."]
[3.15,10.0,"101-3150",13.8,{"$f":"D8*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":25.78673293}]
[2.5,12.0,"101-2500",13.8,25.78673293]
[2.24,13.0,"101-2240",13.8,25.78673293]
[2.0,14.0,"101-2000",13.8,25.78673293]
[1.6,16.0,"101-1600",13.93,26.02965143]
[1.4,17.0,"101-1400",13.93,26.02965143,null,null,null,null,"Galvanised ","Not Polished"]
[1.25,18.0,"101-1250",14.06,26.27256993,null,null,null,null,"Galvanised ","Not Polished"]
[1.12,null,"101-1120",14.06,26.27256993]
[1.0,19.0,"101-1000",14.43,26.96395335,null,null,null,null,"Galvanised ","Not Polished"]
[0.9,20.0,"101-0900",14.73,27.5245345,null,null,null,null,"Galvanised ","Not Polished"]
[0.8,21.0,"101-0800",15.6,29.15021984]
[0.71,22.0,"101-0710",16.8,31.39254444,null,null,null,null,"Galvanised ","Not Polished"]
[0.63,23.0,"101-0630",23.76,44.39802714,null,null,null,null,"Galvanised ","Not Polished"]
[0.56,24.0,"101-0560",24.49,45.76210794,null,null,null,null,"Galvanised ","Not Polished"]
[0.5,25.0,"101-0500",24.8,46.34137512,null,null,null,null,"Galvanised ","Not Polished"]
[0.45,26.0,"101-0450",27.25,50.91945452]
[0.4,27.0,"101-0400",32.77,61.23414769]
[]
[]
[null,null,null,null,"0-1.9"]
[0.355,29.0,"101-0355",34.8,{"$f":"D28*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":65.02741348}]
[0.315,30.0,"101-0315",38.94,72.76343336]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"SURGICAL WIRE SAWS"]
[]
[null,null,null,null,"MATERIAL 316 "]
[]
[]
[null,null,null,null,"S/S FERRULE"]
[null,null,null,null,"CHARNLEY"]
[]
[null,null,"PART NO",null,null,"LENGTH",null,"PRICE"]
[]
[null,null,"730-0030",null,null,"30 cm",null,25.0]
[null,null,"730-0040",null,null,"40 cm",null,25.0]
[null,null,"730-0050",null,null,"50 cm",null,25.0]
[null,null,"730-0070",null,null,"70 cm",null,25.0]
[]
[]
[null,null,null,null,"GIGLI"]
[null,null,null,null,"WITH S/S FERRULES"]
[]
[null,null,"732-0030N",null,null,"30 cm",null,15.0]
[null,null,"732-0040N",null,null,"40 cm",null,12.0]
[null,null,"732-0050N",null,null,"50 cm",null,12.0]
[null,null,"732-0070N",null,null,"70 cm",null,12.0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"STAINLESS STEEL BRAID"]
[null,null,"MATERIAL GRADE 316"]
[]
[]
["CONSTRUCTION",null,null,null,"SIZE",null,"PART NO.",null,"PRICE PER METRE"]
["MM",null,null,null,"MM"]
[]
["16/1/0.2",null,null,null,1.25,null,"113B-1250",null,2.2]
["16/1/0.16",null,null,null,0.9,null,"113B-0900",null,2.37]
["16/1/0.125",null,null,null,0.71,null,"113B-0710",null,2.94]
["16/1/0.1",null,null,null,0.56,null,"113B-0560",null,3.39]
["16/1/0.08",null,null,null,0.45,null,"113B-0450",null,3.96]
["16/1/0.071",null,null,null,0.375,null,"113B-0375",null,4.7]
["16/1/0.63",null,null,null,0.315,null,"113B-0315",null,4.99]
["16/1/0.56",null,null,null,0.28,null,"113B-0280",null,5.15]
["16/1/0.50",null,null,null,0.224,null,"113B-0224",null,5.29]
["8/1/0.063",null,null,null,0.2,null,"113B-0200",null,5.58]
["8/1/0.050",null,null,null,0.16,null,"113B-0160",null,5.73]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"Annealed Stainless Steel Wire"]
[null,null,null,null,"Material Grade 316"]
[]
[null,null,null,null,"X   10   METRE   REELS"]
[]
[]
["SIZE","PART NO.",null,null,"1 to 99",null,"100-249",null,"250-499","500+"]
[]
[1.6,"108B-1600",null,8.0,{"$f":"D146*1.1*1.04*1.05*1.05*1.05*1.05*1.1*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":22.86562775},null,{"$f":"E146*0.9","v":20.57906497},null,{"$f":"E146*0.85","v":19.43578358},{"$f":"E146*0.8","v":18.2925022}]
[1.25,"108B-1250",null,7.28,20.80772125,null,18.72694912,null,17.68656306,16.646177]
[0.9,"108B-0900",null,5.78,16.52041605,null,14.86837444,null,14.04235364,13.21633284]
[0.71,"108B-0710",null,5.2,14.86265803,null,13.37639223,null,12.63325933,11.89012643]
[0.56,"108B-0560",null,4.85,13.86228682,null,12.47605814,null,11.7829438,11.08982946]
[0.45,"108B-0450",null,4.65,13.29064613,null,11.96158151,null,11.29704921,10.6325169]
[0.4,"108B-0400",null,4.65,13.29064613,null,11.96158151,null,11.29704921,10.6325169]
[0.315,"108B-0315",null,4.65,13.29064613,null,11.96158151,null,11.29704921,10.6325169]
[0.28,"108B-0280",null,4.65,13.29064613,null,11.96158151,null,11.29704921,10.6325169]
[0.224,"108B-0224",null,4.65,13.29064613,null,11.96158151,null,11.29704921,10.6325169]
[0.2,"108B-0200",null,4.65,13.29064613,null,11.96158151,null,11.29704921,10.6325169]
[0.16,"108B-0160",null,4.65,13.29064613,null,11.96158151,null,11.29704921,10.6325169]
[0.125,"108B-0125",null,4.65,13.29064613,null,11.96158151,null,11.29704921,10.6325169]
[]
[]
[null,null,"MATERIAL:   ANNEALED POLISHED STAINLESS STEEL",null,null,null,null,null,null,"IMPLANT GRADE"]
[null,null,"Specification:   BS 7252:PART 1:1990"]
[]
[null,null,null,null,"X 10 MTR REELS"]
[]
["SIZE","PART NO.",null,null,"1 to 99",null,"100-249",null,"250-499","500+"]
[]
[1.6,"208B-1600",null,17.9,{"$f":"D168*1.1*1.04*1.05*1.05*1.05*1.07*1.1*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":52.13635336},null,{"$f":"E168*0.9","v":46.92271802},null,{"$f":"E168*0.85","v":44.31590036},{"$f":"E168*0.8","v":41.70908269}]
[1.25,"208B-1250",null,11.9,34.66048073,null,31.19443265,null,29.46140862,27.72838458]
[0.9,"208B-0900",null,8.67,25.25263596,null,22.72737236,null,21.46474056,20.20210877]
[0.71,"208B-0710",null,7.16,20.85454134,null,18.76908721,null,17.72636014,16.68363308]
[0.56,"208B-0560",null,6.36,18.52442499,null,16.67198249,null,15.74576124,14.81953999]
[0.45,"208B-0450",null,5.78,16.83509064,null,15.15158157,null,14.30982704,13.46807251]
[0.4,"208B-0400",null,5.78,16.83509064,null,15.15158157,null,14.30982704,13.46807251]
[0.315,"208B-0315",null,5.78,16.83509064,null,15.15158157,null,14.30982704,13.46807251]
[0.2,"208B-0200",null,5.78,16.83509064,null,15.15158157,null,14.30982704,13.46807251]
[]
[]
[]
[]
[]
[]
[]
[null,null,"ANNEALED POLISHED STAINLESS STEEL WIRE "]
[null,null,"Material Grade 316 "]
[]
[]
[null,null,null,null,"X   25   GRAM   REELS"]
[]
[]
["SIZE",null,"PRICE EACH REEL"]
["MM","PART NO.",null,null,null,"1 to 20","21-60","61-120","120+"]
[]
[1.6,"108A-1600",null,5.78,null,13.66,{"$f":"F194*0.67","v":9.1522},{"$f":"F194*0.6","v":8.196},{"$f":"F194*0.55","v":7.513}]
[1.25,"108A-1250",null,5.78,null,13.66,9.1522,8.196,7.513]
[1.0,"108A-1000",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.9,"108A-0900",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.8,"108A-0800",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.71,"108A-0710",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.63,"108A-0630",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.56,"108A-0560",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.5,"108A-0500",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.45,"108A-0450",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.4,"108A-0400",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.315,"108A-0315",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.28,"108A-0280",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.25,"108A-0250",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.224,"108A-0224",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.2,"108A-0200",null,5.78,null,13.66,9.1522,8.196,7.513]
[0.125,"108A-0125",null,7.51,null,17.22,11.5374,10.332,9.471]
[0.1,"108A-0100",null,9.24,null,20.53,13.7551,12.318,11.2915]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"MATERIAL:  HARD  POLISHED STAINLESS STEEL"]
[null,null,"Material Grade 316"]
[]
["SIZE",null,null,null," SALES PRICE PER KILO"]
["MM","S.W.G.","PART NO.",null,"0-2.9","3-6.9","7-12.9","13-24.9","25+KG"]
[3.15,10.0,"107-3150",24.95,{"$f":"D235*1.04*1.04*1.05*1.05*1.05*1.07*1.15*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":71.82968796},{"$f":"E235*0.9","v":64.64671916},{"$f":"E235*0.8","v":57.46375037},{"$f":"E235*0.6","v":43.09781278},{"$f":"E235*0.55","v":39.50632838}]
[2.5,12.0,"107-2500",24.95,71.82968796,64.64671916,57.46375037,43.09781278,39.50632838]
[2.0,14.0,"107-2000",24.95,71.82968796,64.64671916,57.46375037,43.09781278,39.50632838]
[1.6,16.0,"107-1600",24.95,71.82968796,64.64671916,57.46375037,43.09781278,39.50632838]
[1.4,17.0,"107-1400",25.9,74.5646861,67.10821749,59.65174888,44.73881166,41.01057735]
[1.25,18.0,"107-1250",26.06,75.02531736,67.52278563,60.02025389,45.01519042,41.26392455]
[1.0,19.0,"107-1000",29.45,84.7849423,76.30644807,67.82795384,50.87096538,46.63171827]
[0.9,20.0,"107-0900",29.54,85.04404739,76.53964265,68.03523791,51.02642843,46.77422606]
[0.8,21.0,"107-0800",30.02,86.42594118,77.78334707,69.14075295,51.85556471,47.53426765]
[0.71,22.0,"107-0710",27.52,79.22857766,71.3057199,63.38286213,47.5371466,43.57571771]
[0.63,23.0,"107-0630",30.42,87.57751935,78.81976741,70.06201548,52.54651161,48.16763564]
[0.56,24.0,"107-0560",30.75,88.52757133,79.6748142,70.82205707,53.1165428,48.69016423]
[0.5,25.0,"107-0500",32.12,92.47172654,83.22455389,73.97738123,55.48303593,50.8594496]
[0.45,26.0,"107-0450",32.7,94.14151488,84.72736339,75.3132119,56.48490893,51.77783318]
[0.4,27.0,"107-0400",35.5,102.202562,91.98230582,81.76204962,61.32153722,56.21140911]
[]
[]
[]
[null,null,null,null,"0-1.8","2-3.9","4-6.9","7-12.9","13+KG"]
[0.355,29.0,"107-0355",38.3,{"$f":"D254*1.04*1.04*1.05*1.05*1.05*1.07*1.15*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":110.2636092},{"$f":"E254*0.9","v":99.23724826},{"$f":"E254*0.8","v":88.21088734},{"$f":"E254*0.6","v":66.1581655},{"$f":"E254*0.55","v":60.64498504}]
[0.315,30.0,"107-0315",38.3,110.2636092,99.23724826,88.21088734,66.1581655,60.64498504]
[0.224,34.0,"107-0224",57.02,164.1574672,147.7417205,131.3259738,98.49448034,90.28660698]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"MATERIAL:  ANNEALED POLISHED STAINLESS STEEL"]
[null,null,"Material Grade 316"]
[]
[]
[]
[null,null,null,null,"0-1.8","2-3.9","4-6.9","7-12.9","13+KG"]
[1.6,16.0,"108-1600",27.65,{"$f":"D282*1.04*1.04*1.05*1.05*1.05*1.07*1.15*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":79.60284056},{"$f":"E282*0.9","v":71.64255651},{"$f":"E282*0.8","v":63.68227245},{"$f":"E282*0.6","v":47.76170434},{"$f":"E282*0.55","v":43.78156231}]
[1.25,18.0,"108-1250",29.37,84.55462667,76.099164,67.64370133,50.732776,46.50504467]
[1.0,19.0,"108-1000",31.34,90.22614912,81.20353421,72.1809193,54.13568947,49.62438202]
[0.9,20.0,"108-0900",33.0,95.0051985,85.50467865,76.0041588,57.0031191,52.25285918]
[0.8,21.0,"108-0800",33.5,96.44467121,86.80020409,77.15573697,57.86680272,53.04456916]
[0.71,22.0,"108-0710",34.52,99.38119553,89.44307597,79.50495642,59.62871732,54.65965754]
[0.63,23.0,"108-0630",34.52,99.38119553,89.44307597,79.50495642,59.62871732,54.65965754]
[0.56,24.0,"108-0560",36.43,104.8799813,94.39198313,83.90398501,62.92798875,57.68398969]
[0.5,25.0,"108-0500",37.47,107.8740845,97.08667603,86.29926759,64.72445069,59.33074647]
[0.45,26.0,"108-0450",41.85,120.4838654,108.4354788,96.3870923,72.29031923,66.26612596]
[0.4,27.0,"108-0400",43.63,125.6083882,113.0475494,100.4867106,75.36503292,69.08461351]
[]
[]
[null,null,null,null,"0-0.8","1-1.9","2-3.9","4-6.9","7+KG"]
[0.315,30.0,"108-0315",53.35,{"$f":"D296*1.04*1.04*1.05*1.05*1.05*1.07*1.15*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":153.5917376},{"$f":"E296*0.9","v":138.2325638},{"$f":"E296*0.8","v":122.8733901},{"$f":"E296*0.6","v":92.15504255},{"$f":"E296*0.55","v":84.47545567}]
[0.25,33.0,"108-0250",55.08,158.5723131,142.7150818,126.8578505,95.14338788,87.21477223]
[0.224,34.0,"108-0224",58.94,169.6850424,152.7165382,135.7480339,101.8110255,93.32677333]
[0.2,36.0,"108-0200",62.83,180.8841401,162.7957261,144.707312,108.530484,99.48627703]
[0.125,40.0,"108-0125",81.6,234.9219454,211.4297509,187.9375563,140.9531672,129.20707]
[0.1,42.0,"108-0100",151.83,437.1102815,393.3992533,349.6882252,262.2661689,240.4106548]
[0.071,45.0,"108-0071",195.21,561.9989333,505.79904,449.5991467,337.19936,309.0994133]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"MATERIAL:   ANNEALED POLISHED STAINLESS STEEL",null,null,null,null,null,null,"IMPANT GRADE"]
[null,null,"Specification:   ISO 5832-1 2007"]
[]
["SIZE",null,null,null," SALES PRICE PER KILO"]
["MM","S.W.G.","PART NO.",null,"0-1.9","2-3.9","4-6.9","7-12.9","13+KG"]
[1.6,16.0,"208-1600",70.46,{"$f":"D327*1.05*1.04*1.05*1.05*1.05*1.07*1.15*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.05*1.1*1.1","v":215.041028},{"$f":"E327*0.9","v":193.5369252},{"$f":"E327*0.8","v":172.0328224},{"$f":"E327*0.6","v":129.0246168},{"$f":"E327*0.55","v":118.2725654}]
[1.25,18.0,"208-1250",70.46,215.041028,193.5369252,172.0328224,129.0246168,118.2725654]
[0.9,20.0,"208-0900",72.07,219.9546819,197.9592137,175.9637455,131.9728092,120.9750751]
[0.71,22.0,"208-0710",73.95,225.6923648,203.1231283,180.5538918,135.4154189,124.1308006]
[0.56,24.0,"208-0560",84.9,259.1113153,233.2001838,207.2890523,155.4667892,142.5112234]
[0.45,26.0,"208-0450",88.02,268.6334273,241.7700845,214.9067418,161.1800564,147.748385]
[0.4,27.0,"208-0400",91.28,278.5828135,250.7245321,222.8662508,167.1496881,153.2205474]
[0.315,30.0,"208-0315",96.1,293.2932556,263.9639301,{"$f":"F334*0.9","v":237.567537},213.8107833,192.429705]
[0.25,33.0,"208-0250",100.0,305.1958955,274.676306,{"$f":"F335*0.9","v":247.2086754},222.4878079,200.2390271]
[0.2,36.0,"208-0200",121.28,370.1415821,333.1274239,{"$f":"F336*0.9","v":299.8146815},269.8332134,242.849892]
[0.125,40.0,"208-0125",150.0,457.7938433,412.014459,{"$f":"F337*0.9","v":370.8130131},333.7317118,300.3585406]
[]
[]
[]
[null,null,"MATERIAL:  STAINLESS STEEL LOCKING  WIRE "]
[null,null,"Material Grade 316"]
[]
[null,null,null,null,"X 500 GRM CANS"]
[]
[]
[]
[null,null,null,null,"SALES PRICE PER CAN"]
["MM","S.W.G.","PART NO.",null,"0-4","5 TO 8","9 TO 14","15 TO 26 ","26+"]
[0.8,21.0,"108-CAN-0800",19.48,{"$f":"D350*1.04*1.04*1.05*1.05*1.05*1.07*1.15*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":56.08185657},{"$f":"E350*0.9","v":50.47367091},{"$f":"E350*0.8","v":44.86548526},{"$f":"E350*0.6","v":33.64911394},{"$f":"E350*0.55","v":30.84502111}]
[0.5,25.0,"108-CAN-0500",22.07,63.53832518,57.18449266,50.83066014,38.12299511,34.94607885]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"MATERIAL:  ANNEALED STEEL LOCKING WIRE."]
[null,null,null,null,"SPECIFICATION:  DTD 189A"]
[]
[]
[]
[null,null,null,null,null,"SALES PRICE PER KILO"]
["S.W.G.","PART NO.",null,null,"0-0.9","1-1.9","2-3.9","4-6.9","7+"]
[14.0,"108DTD-2000",null,82.72,{"$f":"D375*1.04*1.04*1.05*1.05*1.05*1.07*1.1*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":227.7921745},{"$f":"E375*0.9","v":205.012957},184.5116613,166.0604952,149.4544457]
[16.0,"108DTD-1600",null,100.0,275.377387,{"$f":"E376*0.9","v":247.8396483},223.0556834,200.7501151,180.6751036]
[18.0,"108DTD-0018",null,83.88,230.9865522,{"$f":"E377*0.9","v":207.887897},{"$f":"E377*0.8","v":184.7892418},{"$f":"E377*0.6","v":138.5919313},{"$f":"E377*0.55","v":127.0426037}]
[20.0,"108DTD-0020",null,83.88,230.9865522,207.887897,184.7892418,138.5919313,127.0426037]
[21.0,"108DTD-0021",null,85.03,234.1533921,210.7380529,187.3227137,140.4920353,128.7843657]
[22.0,"108DTD-0022",null,85.4,235.1722885,211.6550596,188.1378308,141.1033731,129.3447587]
[24.0,"108DTD-0024",null,82.18,226.3051366,203.6746229,181.0441093,135.783082,124.4678251]
[25.0,"108DTD-0025",null,86.9,239.3029493,215.3726543,191.4423594,143.5817696,131.6166221]
[26.0,"108DTD-0026",null,91.4,251.6949317,226.5254385,201.3559454,151.016959,138.4322124]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"MATERIAL:  ANNEALED PLAIN COPPER"]
[null,null,"Material Grade BSEN 13602:2013"]
[]
[]
[]
["SIZE",null,null,null,"SALES PRICE PER KILO"]
["MM","S.W.G.","PART NO.",null,"0-2.9","3-6.9","7-12.9","13-24.9","25+"]
[3.25,10.0,"201-3250",13.3,{"$f":"D421*1.03*1.04*1.05*1.05*1.05*1.05*1.1*1.05*1.5*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":53.39253997},{"$f":"E421*0.9","v":48.05328597},{"$f":"E421*0.8","v":42.71403198},{"$f":"E421*0.6","v":32.03552398},{"$f":"E421*0.55","v":29.36589698}]
[2.5,12.0,"201-2500",13.95,56.00194982,50.40175484,44.80155985,33.60116989,30.8010724]
[2.0,14.0,"201-2000",13.95,56.00194982,50.40175484,44.80155985,33.60116989,30.8010724]
[1.6,16.0,"201-1600",13.68,54.91804111,49.426237,43.93443289,32.95082467,30.20492261]
[1.4,17.0,"201-1400",13.68,54.91804111,49.426237,43.93443289,32.95082467,30.20492261]
[1.25,18.0,"201-1250",13.68,54.91804111,49.426237,43.93443289,32.95082467,30.20492261]
[1.0,19.0,"201-1000",13.68,54.91804111,49.426237,43.93443289,32.95082467,30.20492261]
[0.9,20.0,"201-0900",13.68,54.91804111,49.426237,43.93443289,32.95082467,30.20492261]
[0.8,21.0,"201-0800",13.68,54.91804111,49.426237,43.93443289,32.95082467,30.20492261]
[0.71,22.0,"201-0710",13.33,53.51297427,48.16167684,42.81037942,32.10778456,29.43213585]
[0.61,23.0,"201-0610",13.33,53.51297427,48.16167684,42.81037942,32.10778456,29.43213585]
[0.56,24.0,"201-0560",18.15,72.86275191,65.57647672,58.29020153,43.71765115,40.07451355]
[0.5,25.0,"201-0500",18.2,73.06347575,65.75712817,58.4507806,43.83808545,40.18491166]
[0.45,26.0,"201-0450",18.51,74.30796352,66.87716717,59.44637082,44.58477811,40.86937994]
[0.4,27.0,"201-0400",18.58,74.58897689,67.1300792,59.67118151,44.75338613,41.02393729]
[0.355,29.0,"201-0355",16.75,67.24248455,60.51823609,53.79398764,40.34549073,36.9833665]
[0.3,30.0,"201-0300",15.43,61.94337532,55.74903779,49.55470026,37.16602519,34.06885643]
[0.25,33.0,"201-0250",15.86,63.6696003,57.30264027,50.93568024,38.20176018,35.01828016]
[0.2,36.0,"201-0200",16.7,67.04176071,60.33758464,53.63340857,40.22505643,36.87296839]
[]
[]
[]
[null,null,null,null,"0-0.8","1-1.9","2-3.9","4-6.9","7+"]
[0.15,38.0,"201-0150",15.22,{"$f":"D444*1.03*1.04*1.05*1.05*1.05*1.05*1.1*1.05*1.5*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":61.10033521},{"$f":"E444*0.9","v":54.99030169},{"$f":"E444*0.8","v":48.88026817},{"$f":"E444*0.6","v":36.66020113},{"$f":"E444*0.55","v":33.60518437}]
[0.122,40.0,"201-0122",16.92,67.92494559,61.13245103,54.33995647,40.75496735,37.35872007]
[0.1,42.0,"201-0100",18.04,72.42115948,65.17904353,57.93692758,43.45269569,39.83163771]
[0.08,44.0,"201-0080",30.4,122.0400914,109.8360822,97.63207309,73.22405482,67.12205025]
[0.071,45.0,"201-0071",30.65,123.0437105,110.7393395,98.43496843,73.82622632,67.67404079]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"MATERIAL:  ANNEALED TINNED COPPER"]
[null,null,"Material Grade BSEN 13602:2013"]
[]
[]
[]
["SIZE",null,null,null,"SALES PRICE PER KILO"]
["MM","S.W.G.","PART NO.",null,"0-2.9","3-6.9","7-12.9","13-24.9","25+"]
[2.0,14.0,"202-2000",14.33,{"$f":"D467*1.03*1.04*1.05*1.05*1.05*1.05*1.1*1.05*1.5*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":57.52745096},{"$f":"E467*0.9","v":51.77470586},{"$f":"E467*0.8","v":46.02196077},{"$f":"E467*0.6","v":34.51647058},{"$f":"E467*0.55","v":31.64009803}]
[1.8,15.0,"202-1800",14.33,57.52745096,51.77470586,46.02196077,34.51647058,31.64009803]
[1.6,16.0,"202-1600",14.33,57.52745096,51.77470586,46.02196077,34.51647058,31.64009803]
[1.4,17.0,"202-1400",14.33,57.52745096,51.77470586,46.02196077,34.51647058,31.64009803]
[1.25,18.0,"202-1250",14.33,57.52745096,51.77470586,46.02196077,34.51647058,31.64009803]
[1.0,19.0,"202-1000",14.8,59.414255,53.4728295,47.531404,35.648553,32.67784025]
[0.9,20.0,"202-0900",14.9,59.81570267,53.83413241,47.85256214,35.8894216,32.89863647]
[0.8,21.0,"202-0800",14.96,60.05657127,54.05091415,48.04525702,36.03394276,33.0311142]
[0.71,22.0,"202-0710",15.15,60.81932185,54.73738966,48.65545748,36.49159311,33.45062702]
[0.63,23.0,"202-0630",17.95,72.05985658,64.85387092,57.64788526,43.23591395,39.63292112]
[0.56,24.0,"202-0560",18.22,73.14376528,65.82938875,58.51501223,43.88625917,40.22907091]
[0.5,25.0,"202-0500",18.4,73.86637109,66.47973398,59.09309687,44.31982265,40.6265041]
[0.45,26.0,"202-0450",18.65,74.86999026,67.38299123,59.89599221,44.92199416,41.17849464]
[0.4,27.0,"202-0400",19.62,78.76403265,70.88762938,63.01122612,47.25841959,43.32021796]
[0.375,29.0,"202-0375",19.54,78.44287451,70.59858706,62.75429961,47.06572471,43.14358098]
[0.3,30.0,"202-0300",18.4,73.86637109,66.47973398,59.09309687,44.31982265,40.6265041]
[0.28,32.0,"202-0280",18.6,74.66926642,67.20233978,59.73541314,44.80155985,41.06809653]
[0.25,33.0,"202-0250",18.68,74.99042456,67.4913821,59.99233965,44.99425474,41.24473351]
[]
[]
[]
[null,null,null,null,"0-0.8","1-1.9","2-3.9","4-6.9","7+"]
[0.2,36.0,"202-0200",20.13,{"$f":"D489*1.03*1.04*1.05*1.05*1.05*1.05*1.1*1.05*1.5*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":80.81141576},{"$f":"E489*0.9","v":72.73027418},{"$f":"E489*0.8","v":64.64913261},{"$f":"E489*0.6","v":48.48684946},{"$f":"E489*0.55","v":44.44627867}]
[0.18,37.0,"202-0160",20.68,83.01937794,74.71744014,66.41550235,49.81162676,45.66065787]
[0.15,38.0,"202-0150",20.68,83.01937794,74.71744014,66.41550235,49.81162676,45.66065787]
[0.122,40.0,"202-0122",20.68,83.01937794,74.71744014,66.41550235,49.81162676,45.66065787]
[0.1,42.0,"202-0100",20.9,83.90256281,75.51230653,67.12205025,50.34153769,46.14640955]
[0.071,45.0,"202-0071",22.0,88.31848717,79.48663845,70.65478974,52.9910923,48.57516794]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"MATERIAL :   ANNEALED ALUMINIUM WIRE   99.5%"]
[null,null,"SPECIFICATION:  BS EN 2627"]
[]
[]
[]
["SIZE",null,null,null,"SALES PRICE PER KILO"]
["MM","S.W.G.","PART NO.",null,"0-2.9","3-6.9","7-12.9","13-24.9","25+"]
[3.15,10.0,"306-3150",21.43,{"$f":"D513*1.05*1.04*1.05*1.05*1.05*1.05*1.1*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":58.46715031},{"$f":"E513*0.9","v":52.62043528},{"$f":"E513*0.8","v":46.77372025},{"$f":"E513*0.6","v":35.08029019},{"$f":"E513*0.55","v":32.15693267}]
[2.5,12.0,"306-2500",21.43,58.46715031,52.62043528,46.77372025,35.08029019,32.15693267]
[1.6,16.0,"306-1600",21.43,58.46715031,52.62043528,46.77372025,35.08029019,32.15693267]
[1.22,18.0,"306-1220",21.43,58.46715031,52.62043528,46.77372025,35.08029019,32.15693267]
[0.914,20.0,"306-0914",21.43,58.46715031,52.62043528,46.77372025,35.08029019,32.15693267]
[0.457,26.0,"306-0457",22.58,61.60467821,55.44421039,49.28374257,36.96280692,33.88257301]
[]
[]
[]
["SIZE",null,null,null,"SALES PRICE PER KILO",null,null,null,null,0.9998]
["MM","S.W.G.","PART NO.",null,"0-2.9","3-6.9","7-12.9","13-24.9","25+"]
[1.0,19.0,"307-1000",50.45,{"$f":"D524*1.05*1.04*1.05*1.05*1.05*1.05*1.1*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":137.6419847},{"$f":"E524*0.9","v":123.8777863},{"$f":"E524*0.8","v":110.1135878},{"$f":"E524*0.6","v":82.58519085},{"$f":"E524*0.55","v":75.70309161}]
[]
[]
[]
[null,null,"ANTIMONIAL LEAD 1/99%"]
[null,null,"SPECIFICATION:99% LEAD 1% ANT BS602"]
[]
["SIZE",null,null,null,"SALES PRICE PER KILO"]
["MM","S.W.G","PART NO.",null,"0-2.9","3-6.9","7-12.9","13-24.9","25+"]
[1.6,16.0,"401-1600",10.12,{"$f":"D533*1.05*1.04*1.05*1.05*1.05*1.05*1.1*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":27.6102455},{"$f":"E533*0.9","v":24.84922095},{"$f":"E533*0.8","v":22.0881964},{"$f":"E533*0.6","v":16.5661473},{"$f":"E533*0.55","v":15.18563503}]
[]
[]
[]
[]
[null,null,"MATERIAL:  80/20 NICKEL CHROME"]
[null,null,"Specification:   BSS  115"]
[]
[null,null,null,null," SALES PRICE PER KILO"]
["SIZE"]
["MM","S.W.G.","PART NO.",null,"0-1.9","2-3.9","4-6.9","7-12.9","13+KG"]
[1.6,16.0,"503-1600",85.65,{"$f":"D544*1.05*1.04*1.05*1.05*1.1*1.1*1.1*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":256.4625141},{"$f":"E544*0.9","v":230.8162627},{"$f":"E544*0.8","v":205.1700112},{"$f":"E544*0.6","v":153.8775084},{"$f":"E544*0.55","v":141.0543827}]
[0.9,20.0,"503-0900",87.04,260.6246027,234.5621425,208.4996822,156.3747616,143.3435315]
[0.71,22.0,"503-0710",87.82,262.9601633,236.6641469,210.3681306,157.776098,144.6280898]
[0.56,24.0,"503-0560",95.39,285.6270778,257.06437,228.5016623,171.3762467,157.0948928]
[0.45,26.0,"503-0450",101.2,303.0240096,272.7216086,242.4192077,181.8144058,166.6632053]
[]
[]
[]
[null,null,"MATERIAL:  ANNEALED PURE NICKEL 200"]
[null,null,"Specification:   BSS 3075 N.A.11"]
[]
[]
["SIZE",null,null,null," SALES PRICE PER KILO"]
["MM","S.W.G.","PART NO.",null,"0-2.9","3-6.9","7-12.9","13-24.9","25+"]
[1.6,16.0,"505-1600",76.04,{"$f":"D558*1.03*1.04*1.05*1.05*1.1*1.1*1.1*1.05*1.05*1.05*1.05*1.1*1.05*1.1*1.1","v":203.0457374},{"$f":"E558*0.9","v":182.7411637},{"$f":"E558*0.8","v":162.4365899},{"$f":"E558*0.6","v":121.8274424},{"$f":"E558*0.55","v":111.6751556}]
[1.0,19.0,"505-1000",76.04,203.0457374,182.7411637,162.4365899,121.8274424,111.6751556]
[0.45,26.0,"505-0450",77.84,207.8521857,187.0669671,166.2817485,124.7113114,114.3187021]
[]
[]
[]
[null,null,"MATERIAL:  ANNEALED MONEL 400"]
[null,null,"Specification:   BSS 3075 NA / 13"]
[]
[]
["SIZE",null,null,null," SALES PRICE PER KILO"]
["MM","S.W.G.","PART NO.",null,"0-2.9","3-6.9","7-12.9","13-24.9","25+"]
[1.6,16.0,"508-1600",57.44,{"$f":"D570*1.03*1.04*1.05*1.05*1.1*1.1*1.1*1.05*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":168.7170157},{"$f":"E570*0.9","v":151.8453141},{"$f":"E570*0.8","v":134.9736125},{"$f":"E570*0.6","v":101.2302094},{"$f":"E570*0.55","v":92.79435862}]
[0.9,20.0,"508-0900",57.17,167.9239517,151.1315565,134.3391614,100.754371,92.35817344]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"PHOSPHOR BRONZE CLOCK CORD"]
[]
[null,null,null,null,"CONSTRUCTION: 5/7/0.18MM"]
[]
[]
[null,"1.4 MM","300-1400",null,null,null,null,null,2.05]
[]
[]
[null,null,null,null,"BLACK POLYPROP COVERED GALVANISED ROPE"]
[]
[null,null,null,null,"CONSTRUCTION: 2 MM 7X7  TO 3 MM"]
[null," 3 MM","713-3000",null,null,null,null,null,1.98]
[]
[null,null,"MATERIAL: GALVANISED ANNEALED MILD STEEL"]
[null,null,"Specification:   BS  1052"]
[]
["SIZE",null,null,null," SALES PRICE PER KILO"]
["MM","S.W.G.","PART NO.",null,"0-2.9","3-6.9","7-12.9","13-24.9","25+KG"]
[3.15,10.0,"905-3150",6.44,{"$f":"D603*1.05*1.04*1.05*1.05*1.05*1.05*1.1*1.05*1.25*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":21.96269529},{"$f":"E603*0.9","v":19.76642576},{"$f":"E603*0.8","v":17.57015623},{"$f":"E603*0.6","v":13.17761717},{"$f":"E603*0.55","v":12.07948241}]
[2.0,14.0,"905-2000",6.9,23.53145924,21.17831331,18.82516739,14.11887554,12.94230258]
[1.6,16.0,"905-1600",7.14,24.34994477,21.9149503,19.47995582,14.60996686,13.39246963]
[1.25,18.0,"905-1250",7.9,26.94181565,24.24763408,21.55345252,16.16508939,14.81799861]
[1.0,19.0,"905-1000",9.0,30.6932077,27.62388693,{"$f":"F607*0.9","v":24.86149824},22.37534841,20.13781357]
[0.87,null,"905-0870",9.0,30.6932077,27.62388693,{"$f":"F608*0.9","v":24.86149824},22.37534841,20.13781357]
[]
[]
[]
[]
[null,null,"MATERIAL: BLACK ANNEALED MILD STEEL"]
[null,null,"Specification:   BS  1052"]
["SIZE"]
["MM",null,null,null," SALES PRICE PER KILO"]
[null,"S.W.G.","PART NO.",null,"0-2.9","3-6.9","7-12.9","13-24.9","25+KG"]
[3.15,10.0,"904-3150",5.68,{"$f":"D618*1.05*1.04*1.05*1.05*1.05*1.05*1.1*1.05*1.45*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":22.47015632},{"$f":"E618*0.9","v":20.22314069},{"$f":"E618*0.8","v":17.97612506},{"$f":"E618*0.6","v":13.48209379},{"$f":"E618*0.55","v":12.35858598}]
[2.0,14.0,"904-2000",5.69,22.50971646,20.25874481,18.00777316,13.50582987,12.38034405]
[1.6,16.0,"904-1600",5.91,23.38003941,21.04203547,{"$f":"F620*0.9","v":18.93783192},17.04404873,15.33964386]
[1.25,18.0,"904-1250",5.94,23.49871981,21.14884783,{"$f":"F621*0.9","v":19.03396305},17.13056674,15.41751007]
[1.0,19.0,"904-1000",5.94,23.49871981,21.14884783,{"$f":"F622*0.9","v":19.03396305},17.13056674,15.41751007]
[]
[0.71,22.0,"904-0710",5.94,{"$f":"D624*1.05*1.04*1.05*1.05*1.05*1.05*1.1*1.05*1.45*1.05*1.05*1.05*1.1*1.1*1.05*1.1*1.1","v":23.49871981},{"$f":"E624*0.9","v":21.14884783},19.03396305,17.13056674,15.41751007,"BRIGHT, NOT BLACK"]